**Section 535.240 Certification of Equipment**

A public utility, independent contractor, or their agents shall follow the manufacturer’s testing, maintenance, and certification recommendations for all mercury vapor testing equipment used to test for the presence of mercury vapor and shall keep the records of such testing, maintenance and certifications for five years after its last mercury vapor test required by Section 535.200.