**Section 442.213 Bumper, Rear**

a) The entire rear bumper must be of metal construction unless an energy absorbing bumper is used.

b) The rear bumper must meet chassis or body manufacturer's standards.

c) The rear bumper shall be shielded between the body and the bumper to prevent hitching or "riding on."

AGENCY NOTE: See Section 442.420 for front bumper requirements.

(Source: Added at 26 Ill. Reg. 3255, effective February 19, 2002)