**Section 442.420 Bumper, Front**

a) The front bumper shall meet the chassis manufacturer's standards.

b) The entire front bumper must be of metal construction unless an energy absorbing bumper is used.

AGENCY NOTE: See Section 442.213 for rear bumper requirements.

(Source: Amended at 26 Ill. Reg. 3255, effective February 19, 2002)