**Section 442.460 Ignition Lock**

A key type lock or other device shall be provided to prevent the vehicle from being set in motion or its engine started by unauthorized persons.