**Section 442.465 Instruments**

The bus shall be equipped with the following nonglare illuminated instruments and gauges mounted for easy maintenance and repair and in such a manner that each is clearly visible to the seated operator. An indicator light in lieu of a pressure or temperature gauge is permissible.

a) Speedometer

b) Odometer

c) Fuel Gauge

d) Oil Pressure Gauge

e) Water Temperature Gauge

f) Ampere Meter or Volt Meter with graduated charge and discharge indications

(Source: Amended at 31 Ill. Reg. 8238, effective May 25, 2007)