**Section 448.APPENDIX D Driver Education Training Cars**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 17.1 | In addition to the general testing requirements of Appendix A, driver education training cars are also subject to the following requirements. | | | |
| 17.2 | BRAKES  Vehicles equipped with automatic transmissions shall be equipped with a dual brake. Vehicles equipped with standard transmissions shall be equipped with a dual brake and a dual clutch. ("Dual" means two identical sets of controls – one operable by the driver and the other by a front seat passenger.) | | | |
| PROCEDURE – BRAKES | | | REJECT VEHICLE IF: | |
|  | A. | Test dual brake system in accordance with procedures outlined in Appendix A of these Rules. | A. | Not equipped with a dual system or dual system is inoperative. Dual brake system does not meet the standards outlined in Appendix A. |
| 17.3 | IDENTIFICATION.  The motor vehicle must be equipped with a sign or signs visible from the front and the rear in letters no less than 2 inches tall, listing the full name of the driver training school which has registered and insured the motor vehicle. | | | |
| PROCEDURE – IDENTIFICATION | | | REFJECT VEHICLE IF: | |
|  | A. | Visually check sign or signs. | A. | Sign(s) not provided or not visible from front and rear. |
| 17.4 | EMERGENCY WARNING DEVICES.  Driver Education Training Cars do not require emergency warning devices. | | | |
| 17.5 | MIRRORS  Effective July 1, 1988, Driver Education Training Cars require a mirror on each side of the vehicle so located as to reflect to the driver a view of the highway for a distance of at least 200 feet to the rear of the vehicle. | | | |
| 17.6 | If a Driver Education Training Car meets or exceeds the minimum standards outlined in this Part, a Certificate of Safety must be affixed in the location prescribed in 92 Ill. Adm. Code 448.100. | | | |

(Source: Amended at 12 Ill. Reg. 11566, effective June 23, 1988)