**Section 532.330 Turnout Dimensions**

Standard mailbox turnouts will have the dimensions shown on Illustration A with maximum width (up to 8 feet) the roadway shoulder will accommodate.