**Section 550.ILLUSTRATION F Commercial-Urban**



When the island between drives is less than 25 feet long or less than 10 feet wide, it shall be defined by curves, masonry, or other devices.

\*45º min. angle permitted only for one-way driveways.

60º min. angle for two-way driveways.