**Section 1500.120 Tracks Adjacent to Main Tracks**

a) Except as to ladder tracks, the distance from the centerline of any main track to the centerline of any adjacent subsidiary track shall be not less than 15 feet.

b) The distance from the centerline of any main track to the centerline of any adjacent ladder track in which switches are operated mechanically shall be not less than 15 feet; in ladder tracks where switches are not operated mechanically, 17 feet.

(Source: Amended at 29 Ill. Reg. 20360, effective December 15, 2005)