**Section 1535.347 Painting**

The mast and signal shall be white or aluminum in color. The backgrounds and hoods for the lamp units shall be black, preferably a dull finish.